**Light Sources:**

18pcsx12W W+A 2in1 5050 led (A：1700K, W:6500K)

Beam Angle: 15-55 degree

Power Voltage: AC 100-240V, 50/60Hz

Max Power Consumption: 230W

**Control**DMX Channel:3/5/ 7 Channel
Control Modes: DMX512/Master-Slave/Auto run/music

**Construction**Display: LED Display
Data In/Out socket: 3-pin XLR sockets
Power Socket: PowerCon in and out Power socket

Protection Rating: IP20

**Features**

Dimming :0-100% linear dimming (No flicker)

Support RDM function

High output lens bring surprising brightness

Temperature sense cooling fan (reduce fan noise maximumly)

**Dimension**

Fixture size:220\*230\*290mm; NW: 4.5 kgs

Carton package:29x29x31 cm (1pc/CTN); GW:5 kgs